**PREFACE**

|  |  |
| --- | --- |
| Read this manual keeping in mind that the infor- mation contained here in does not cover every possible contingency to be met with the operation. The operations not described in this manual should not be attended with the control.  The functions and performance as NC machine are determined by a combination of machine and the NC control. For operation of your NC machine, the machine tool builder's manual shall take pri- ority over this manual. | Unless otherwise specified, the following rules apply to the description of programming exam -ples shown in this manual.   * Least Input Increment: 0.01 mm * Feed Function Selection: G94 (mm/min.) * Absolute Zero Point: * Reference Zero Point   (Return to reference zero by manual and auto-  matic return ):   * Dimensions: in MM |

|  |  |
| --- | --- |
| **TABLE OF CONTENTS** | |
| 1. **INTRODUCTION** *1* 2. **PROGRAMMING** *1*    1. Input Format *1*    2. Program Number and Sequence Number *6*    3. Coordinate Word *6*    4. Traverse and Feed Functions *9*    5. Spindle-Speed Function (S -Function) *13*    6. Tool Function (T-Function) *13*    7. Tool Compensation *14*    8. Miscellaneous Functions (M-Function] *15*    9. Preparatory Function (G-Function) *21*    10. User Message Display/ *83*    11. User Macro (G65 and G66) *84* 3. **PART PROGRAM TAPE CODING** *110*    1. Tape Code *110*    2. Programming *110*    3. NC Tape Punching *113*    4. NC Tape *113* 4. **NC OPERATOR'S STATION WITH CRT CHARACTER DISPLAY** *114*    1. Pushbuttons, Lamps and Keys *114*    2. Power On /Off Operation *119*    3. Display and Writing Operation *120*    4. Tape Input/Output Operations of NC DATA *132*    5. Loading Part Programs Into Memory *135*    6. Edit *138*    7. Data Input /Output Interface *140*    8. Tape Verifying *145* 5. **TAPE READER** *148*    1. Tape Reader Compartment *148*    2. Tape Reels *149* | 1. **MACHINE CONTROL STATION** *155*    1. Switching Units on the Control Station *155*    2. Operation Procedure *163* 2. **OPERATION PROCEDURE**    1. Inspection Before Turning on Power *173*    2. Turning on Power *173*    3. Manual Operation *173*    4. Preparation for Stored Leadscrew Error Compensation and Stored Stroke Limit' *173*    5. Preparation for Automatic Operation *173*    6. Operation in Tape and Memory Mode *175*    7. Manual Operation Interrupting Automatic Operation *175*    8. Automatic Operation in MDI Mode *175*    9. MDI Operation Interrupting Automatic Operation *176*    10. Preparation for Turning Off Power *1*76    11. Turning Off Power *176* 3. **MAINTENANCE** 178    1. Routine Inspection Schedule *1* 78    2. Battery Replacement *181*    3. Power Circuit Breaker and Fuses *182*    4. Thermal overload Relay of Servo Unit 184    5. Others *185*    6. Trouble Causes and Remedies *185*   APPENDIX – 1 LIST OF SETTING NUMBERS *187*  APPENDIX – 2 LIST OF PARAMETER NUMBERS *192*  APPENDIX – 3 STORED LEADSCREW ERROR  COMPENSATION *209*  APPENDIX - 4 LIST OF STANDARD INPUT/  OUTPUTSIGNALS *213*  APPENDIX - 5 LIST OF ALARM CODES *222*  APPENDIX - 6 LIST OF ADDRESS CHARACTERS *234* |