**INDEX**

**Subject Chapter** **Section Page**

1. Program Restart 6 6.2.4 167

PUSHBUTTONS, LAMPS AND KEYS 4 4.1 114

1. Rapid Traverse Rate 2 2.4.1 9

RAPID TRAVERSE RATE OVERRIDE Switch 6 6.1.11 157

Reference Point Check (G27) † 2 2.9.13 33

REFERENCE POINT Lamps† 6 6.1.16 159

Reference Point Return (G30) † 2 2.9.16 36

Registration of User Macros 2 2.11.7 101

Registered Program Number, Display of 4 4.5.4 137

Remote Power On/Off Pushbuttons 4 4.2.3 120

RESET Key 4 4.1.12 118

Return from Reference Zero (G29) † 2 2.9.15 35

ROUTINE INSPECTION SCHEDULE 8 8.1 178

1. S2-Digit Programming 2 2.5.1 13

S5-Digit Programming† 2 2.5.2 13

Scaling Function (G50, G51) † 2 2.9.24 60

Sequence Number 2 2.2.2 6

Servomotor and DC Motor for Spindle 8 8 .1.3 179

Setting and Parameter Tape Verifying 4 4.8.1 145

Setting Data and Parameter Data, Inputting 4 4.4.2 133

Setting Data and Parameter Data to Paper Tape. Outputting 4 4 .4.4 133

Setting Data. Displaying and Writing 4 4.3.6 127

SETTING NUMBERS, LIST OF APPENDIX 1 187

Setting of Baud Rate and Others of Serial Interface 4 4.7.3 141

Simultaneously Controllable Axes of Four-axis Control† 2 2.3.3 7

Simultaneously Controllable Axes of. Three-axis Control 2 2.3.2 7

SINGLE BLOCK Switch 6 6.1.17 159

Skip Function (G31) † 2 2.9.17 36

SPINDLE SPEED OVERRIDE Switch † 6 6.1.14 159

SPINDLE-SPEED FUNCTION (S-FUNCTION) 2 2.5 I3

Splicing NC Tape 3 3.4.1 113

STANDARD INPUT/OUTPUT SIGNALS, LIST OF APPENDIX 4 213

START LOCK Input (or Switch) † 6 6.1.27 162

STORED LEADSCREW ERROR COMPENSATION APPENDIX 3 209

STORED LEADSCREW ERROR COMPENSATION AND

STORED STROKE LIMIT †, PREPARATION FOR 7 7.4 173

Stored Stroke Limit (G22, G23) † 2 2.9.12 32

Subroutine Program (M98, M99) 2 2.8.7 19

SWITCHING UNITS ON THE CONTROL STATION 6 6.1 155

1. T2-Digit Programming 2 2.6.1 14

T4-Digit Programming† 2 2.6.2 14

Tape Feed Switch and System No. Switch 5 5.1.1 148

TAPE AND MEMORY MODE, OPERATION IN 7 7.6 175

Tape Code 3 3.1.1 110

TAPE CODE 3 3.1 110

TAPE FEED and SYSTEM No. Switches 4 4.1.13 118

TAPE INPUT /OUTPUT OPERATIONS OF NC DATA 4 4.4 132

Tape Reader 5 5.1.2 148

Tape Reader 8 .8.1.1 179

TAPE READER 5 148

TAPE READER COMPARTMENT 5 5.1 148

Tape Reels, Handling 8-inch 5. 5.2.2 149

Tape Reels, Handling 6-inch 5 .5.2.1 149

TAPE REELS† 5 5.2 149

vi