**INDEX**

**Subject Chapter Section Page**

1. EDIT 4 4.6 138

EDIT Keys 4 4.1.10 117

EDIT LOCK Switch 6 6.1.28 162

Editing Operation, Summary of 4 4.8.4 146

EIA/ISO Auto-Recognition 3 3.1.2 110

EMERGENCY STOP Pushbutton 6 6.1.4 155

Exact Stop (G09, G61, G64) 2 2.9.7 27

Exercises of User Macro 2 2.11.11 105

EXTERNAL DECELERATION Input Signals † 26 6.1.30 162

1. F1-Digit Programming † 2 2.4.4 11

Feed Function Designation (G94, G95) † 1 2 2.9.32 80

FEED HOLD Pushbutton and Lamp 6 6.1.3 155

Feed Per Revolution† 2 2.4.5 12

Feedrate (F-Function) 2 2.4.2 1Q

Feedrate 1/10 2 2.4.3 11

FEEDRATE OVERRIDE CANCEL Switch 6 6.1.13 159

FEEDRATE OVERRIDE Switch 6 6.1.12 157

FUNCTION Keys 4 4.1.3 115

Fuse Blowing (Alarm No. 331, 332) 8 8.4.1 184

Fuse for Servo Control Power Unit 8 8.3.4 183

Fuses of Composite Control Power Supply Unit 8 8.3.2 182

Fuses of Power Input Unit 8 8.3.3 183

1. G Codes and Groups, List of 2 2.9.1 21

(GOO, G06) Positioning 2 2.9.2 23

(G01) Linear Interpolation 2 2.9.3 Z3

(G02, G03) Circular Interpolation 2 2.9.4 24

(G02, G03) † Helical Interpolation 2 2.9.5 26

(G04) Dwell 2 2.9.6 27

(G09, G61, G64) Exact Stop 2 2.9.7 27

(G10) Tool Offset Value Designation 2 2.9.8 28

(G12, G13) † Circle Cutting 2 2.9.9 28

(G17, G18, G19) Plane Designation 2 2.9.10 31

(G20, G21) † Inch/Metric Designation by G Code 2 2.9.11 31

(G22, G23) † Stored Stroke Limit 2 2.9.12 32

(G27) Reference Point Check 2 2.9.13 33

(G28) † Automatic Return to Reference Point 2 2.9.14 34

(G29) † Return from Reference Zero 2 2.9.15 35

(G30) † Reference Point Return 2 2.9.16 36

(G31) † Skip Function 2 2.9.17 36

(G33) † Thread cutting 2 2.9.18 37

(G36, G37) Automatic Centering Function 2 2.9.19 37

(G38) † Z-Axis Reference Surface Offset 2 2.9.20 39

(G40, G41, G 4 2 ) † Tool Radius Compensation C 2 2.9.21 39

(G43, G44, G49) † Tool Length Compensation 2 2.9.22 53

(G45 to G48) Tool Position Offset 22 2.9.23 55

(G50, G51) † Scaling Function 2 2.9.24 60

(G52 to G59) † Work Coordinate System Setting 2 2.9.25 62

(G60) † Unidirectional Approach 2 2.9.26 64

(G70, G71, G72) Hole Pattern Cycles 2 22.9.7 65

(G73, G74, G76, G80 to G89, G98, G99) † Canned Cycles 2 2.9.29 68

(G80, G81) † Output for External Motion 2 2.9.28 67

(G90/G9I) Absolute/Incremental Programming 2 2.9.30 79

(G 92) Programming of Absolute Zero Point 2 2.9.31 79

(G94, G95) † Feed Function Designation 2 2.9.32 80

(G100 through 102) High-Speed Cutting Feature 2 2.9.33 80

iii